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	#
	Original Text
	Change
	Justification

	
1
	§ 7.4.5a) Friable Materials. One (1) blank slide shall be prepared daily or with every fifty (50) samples analyzed, whichever is less.

	DS; § 7.4.5a)  Friable Materials:  Each analyst shall prepare one (1) initial blank slide and one (1) additional blank slide every fifty (50) samples analyzed thereafter per day.
	Language could or has been interpreted such that laboratories are not analyzing a sufficient number of blanks by each analyst each day.

	2
	 Current EL-V1M3 calls for use of NIST standard 2063a which is currently unavailable. See § 7.2.1.1e)iii

	No change in language but reference to Annex for substitute SRM materials hs been added.
	  DS; 7.2.1.1e)iii now reads: 
 “NIST SRM 2063a or similar standard (see Annex A)…”



